;/*++
;INX_COPYRIGHT_1
;INX_COPYRIGHT_2
;
;Module Name:
;    netkvm.inf
;
;Abstract:
;    VirtIO Ethernet Adapter
;
;Installation Notes:
;    Using Devcon: Type "devcon install netkvm.inf PCI\VEN_1AF4&DEV_1000&SUBSYS_0001_INX_SUBSYS_VENDOR_ID&REV_00" or
;                       "devcon install netkvm.inf PCI\VEN_1AF4&DEV_1041&SUBSYS_1100_INX_SUBSYS_VENDOR_ID&REV_01" to install
;
;--*/

[version]
Signature   = "$Windows NT$"
Class       = Net
CatalogFile = netkvm.cat
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %VENDOR%
DriverVer=01/01/2008,0.0.0.1 ; this line will be replaced with stampinf
DriverPackageType = PlugAndPlay
DriverPackageDisplayName = %kvmnet5.DeviceDesc%

[Manufacturer]
%VENDOR% = NetKVM, NT$ARCH$

[NetKVM.NT$ARCH$]
%kvmnet5.DeviceDesc%    = kvmnet5.ndi, PCI\VEN_1AF4&DEV_1000&SUBSYS_0001_INX_SUBSYS_VENDOR_ID&REV_00, PCI\VEN_1AF4&DEV_1000
%kvmnet5.DeviceDesc%    = kvmnet5.ndi, PCI\VEN_1AF4&DEV_1041&SUBSYS_1100_INX_SUBSYS_VENDOR_ID&REV_01, PCI\VEN_1AF4&DEV_1041


[kvmnet5.ndi]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType     = 5 ; PCI
AddReg          = kvmnet5.Reg, Parameters
CopyFiles       = kvmnet5.CopyFiles
*IfType         = 6
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 0      ; NdisPhysicalMediumUnspecified


[kvmnet5.ndi.Services]
AddService      = netkvm, 2, kvmnet5.Service, kvmnet5.EventLog


[kvmnet5.Reg]
HKR,    ,                         BusNumber,           0, "0" 
HKR, Ndi,                         Service,             0, "netkvm"
HKR, Ndi\Interfaces,              UpperRange,          0, "ndis5"
HKR, Ndi\Interfaces,              LowerRange,          0, "ethernet"

[Parameters]
HKR, Ndi\Params\ConnectRate,        ParamDesc,  0,          %ConnectRate%
HKR, Ndi\Params\ConnectRate,        Default,    0,          "1001"
HKR, Ndi\Params\ConnectRate,        type,       0,          "enum"
HKR, Ndi\Params\ConnectRate\enum,   "10",       0,          %10M%
HKR, Ndi\Params\ConnectRate\enum,   "100",      0,          %100M%
HKR, Ndi\Params\ConnectRate\enum,   "1001",     0,          %1G%
HKR, Ndi\Params\ConnectRate\enum,   "10000",    0,          %10G%

HKR, Ndi\Params\Priority,           ParamDesc,  0,          %Priority%
HKR, Ndi\Params\Priority,           Default,    0,          "1"
HKR, Ndi\Params\Priority,           type,       0,          "enum"
HKR, Ndi\Params\Priority\enum,      "1",        0,          %Enable%
HKR, Ndi\Params\Priority\enum,      "0",        0,          %Disable%

HKR, Ndi\Params\*PriorityVLANTag,           ParamDesc,  0,          %PriorityVlanTag%
HKR, Ndi\Params\*PriorityVLANTag,           Default,    0,          "3"
HKR, Ndi\Params\*PriorityVLANTag,           type,       0,          "enum"
HKR, Ndi\Params\*PriorityVLANTag\enum,      "3",        0,          %Priority_Vlan%
HKR, Ndi\Params\*PriorityVLANTag\enum,      "2",        0,          %VLan%
HKR, Ndi\Params\*PriorityVLANTag\enum,      "1",        0,          %PriorityOnly%
HKR, Ndi\Params\*PriorityVLANTag\enum,      "0",        0,          %Disable%

HKR, Ndi\Params\DoLog,              ParamDesc,  0,          %EnableLogging%
HKR, Ndi\Params\DoLog,              Default,    0,          "1"
HKR, Ndi\Params\DoLog,              type,       0,          "enum"
HKR, Ndi\Params\DoLog\enum,         "1",        0,          %Enable%
HKR, Ndi\Params\DoLog\enum,         "0",        0,          %Disable%

HKR, Ndi\params\DebugLevel,         ParamDesc,  0,          %DebugLevel%
HKR, Ndi\params\DebugLevel,         type,       0,          "int"
HKR, Ndi\params\DebugLevel,         default,    0,          "0"
HKR, Ndi\params\DebugLevel,         min,        0,          "0"
HKR, Ndi\params\DebugLevel,         max,        0,          "8"
HKR, Ndi\params\DebugLevel,         step,       0,          "1"

HKR, Ndi\params\LogStatistics,      ParamDesc,  0,          %LogStatistics%
HKR, Ndi\params\LogStatistics,      type,       0,          "int"
HKR, Ndi\params\LogStatistics,      default,    0,          "0"
HKR, Ndi\params\LogStatistics,      min,        0,          "0"
HKR, Ndi\params\LogStatistics,      max,        0,          "10000"
HKR, Ndi\params\LogStatistics,      step,       0,          "1"

HKR, Ndi\params\MTU,                ParamDesc,  0,          %MTU%
HKR, Ndi\params\MTU,                type,       0,          "long"
HKR, Ndi\params\MTU,                default,    0,          "1500"
HKR, Ndi\params\MTU,                min,        0,          "500"
HKR, Ndi\params\MTU,                max,        0,          "65500"
HKR, Ndi\params\MTU,                step,       0,          "1"

HKR, Ndi\params\TxCapacity,         ParamDesc,  0,          %TxCapacity%
HKR, Ndi\params\TxCapacity,         type,       0,          "enum"
HKR, Ndi\params\TxCapacity,         default,    0,          "1024"
HKR, Ndi\Params\TxCapacity\enum,    "16",       0,          %String_16%
HKR, Ndi\Params\TxCapacity\enum,    "32",       0,          %String_32%
HKR, Ndi\Params\TxCapacity\enum,    "64",       0,          %String_64%
HKR, Ndi\Params\TxCapacity\enum,    "128",      0,          %String_128%
HKR, Ndi\Params\TxCapacity\enum,    "256",      0,          %String_256%
HKR, Ndi\Params\TxCapacity\enum,    "512",      0,          %String_512%
HKR, Ndi\Params\TxCapacity\enum,    "1024",     0,          %String_1024%

HKR, Ndi\params\RxCapacity,         ParamDesc,  0,          %RxCapacity%
HKR, Ndi\params\RxCapacity,         type,       0,          "enum"
HKR, Ndi\params\RxCapacity,         default,    0,          "256"
HKR, Ndi\Params\RxCapacity\enum,    "16",       0,          %String_16%
HKR, Ndi\Params\RxCapacity\enum,    "32",       0,          %String_32%
HKR, Ndi\Params\RxCapacity\enum,    "64",       0,          %String_64%
HKR, Ndi\Params\RxCapacity\enum,    "128",      0,          %String_128%
HKR, Ndi\Params\RxCapacity\enum,    "256",      0,          %String_256%
HKR, Ndi\Params\RxCapacity\enum,    "512",      0,          %String_512%
HKR, Ndi\Params\RxCapacity\enum,    "1024",     0,          %String_1024%

HKR, Ndi\Params\MergeableBuf,       ParamDesc,  0,          %MergeableBuf%
HKR, Ndi\Params\MergeableBuf,       Default,    0,          "1"
HKR, Ndi\Params\MergeableBuf,       type,       0,          "enum"
HKR, Ndi\Params\MergeableBuf\enum,  "1",        0,          %Enable%
HKR, Ndi\Params\MergeableBuf\enum,  "0",        0,          %Disable%

HKR, Ndi\params\NetworkAddress,     ParamDesc,  0,          %NetworkAddress%
HKR, Ndi\params\NetworkAddress,     type,       0,          "edit"
HKR, Ndi\params\NetworkAddress,     Optional,   0,          "1"

HKR, Ndi\Params\Indirect,           ParamDesc,  0,          %Indirect%
HKR, Ndi\Params\Indirect,           Default,    0,          "0"
HKR, Ndi\Params\Indirect,           type,       0,          "enum"
HKR, Ndi\Params\Indirect\enum,      "0",        0,          %Disable%
HKR, Ndi\Params\Indirect\enum,      "1",        0,          %Enable%
HKR, Ndi\Params\Indirect\enum,      "2",        0,          %Enable*%

HKR, Ndi\Params\OffLoad.TxChecksum, ParamDesc,  0,          %OffLoad.TxChecksum%
HKR, Ndi\Params\OffLoad.TxChecksum, Default,    0,          "0"
HKR, Ndi\Params\OffLoad.TxChecksum, type,       0,          "enum"
HKR, Ndi\Params\OffLoad.TxChecksum\enum,    "31",       0,  %All%
HKR, Ndi\Params\OffLoad.TxChecksum\enum,    "27",       0,  %TCPUDPAll%
HKR, Ndi\Params\OffLoad.TxChecksum\enum,    "3",        0,  %TCPUDPv4%
HKR, Ndi\Params\OffLoad.TxChecksum\enum,    "1",        0,  %TCPv4%
HKR, Ndi\Params\OffLoad.TxChecksum\enum,    "0",        0,  %Disable%

HKR, Ndi\Params\OffLoad.TxLSO,      ParamDesc,  0,          %OffLoad.TxLSO%
HKR, Ndi\Params\OffLoad.TxLSO,      Default,    0,          "2"
HKR, Ndi\Params\OffLoad.TxLSO,      type,       0,          "enum"
HKR, Ndi\Params\OffLoad.TxLSO\enum, "2",        0,          %Maximal%
HKR, Ndi\Params\OffLoad.TxLSO\enum, "1",        0,          %IPv4%
HKR, Ndi\Params\OffLoad.TxLSO\enum, "0",        0,          %Disable%

HKR, Ndi\Params\OffLoad.RxCS,       ParamDesc,  0,          %OffLoad.RxCS%
HKR, Ndi\Params\OffLoad.RxCS,       Default,    0,          "0"
HKR, Ndi\Params\OffLoad.RxCS,       type,       0,          "enum"
HKR, Ndi\Params\OffLoad.RxCS\enum,  "31",       0,          %All%
HKR, Ndi\Params\OffLoad.RxCS\enum,  "27",       0,          %TCPUDPAll%
HKR, Ndi\Params\OffLoad.RxCS\enum,  "3",        0,          %TCPUDPv4%
HKR, Ndi\Params\OffLoad.RxCS\enum,  "1",        0,          %TCPv4%
HKR, Ndi\Params\OffLoad.RxCS\enum,  "0",        0,          %Disable%

HKR, Ndi\params\ConnectTimer,       ParamDesc,  0,          %ConnectAfter%
HKR, Ndi\params\ConnectTimer,       type,       0,          "long"
HKR, Ndi\params\ConnectTimer,       default,    0,          "0"
HKR, Ndi\params\ConnectTimer,       min,        0,          "0"
HKR, Ndi\params\ConnectTimer,       max,        0,          "300000"
HKR, Ndi\params\ConnectTimer,       step,       0,          "50"

HKR, Ndi\Params\DpcCheck,           ParamDesc,  0,          %DPCCheck%
HKR, Ndi\Params\DpcCheck,           Default,    0,          "0"
HKR, Ndi\Params\DpcCheck,           type,       0,          "enum"
HKR, Ndi\Params\DpcCheck\enum,      "1",        0,          %Enable%
HKR, Ndi\Params\DpcCheck\enum,      "0",        0,          %Disable%
HKR, Ndi\Params\DpcCheck\enum,      "2",        0,          %Enable*%

HKR, Ndi\Params\Gather,             ParamDesc,  0,          %Gather%
HKR, Ndi\Params\Gather,             Default,    0,          "1"
HKR, Ndi\Params\Gather,             type,       0,          "enum"
HKR, Ndi\Params\Gather\enum,        "1",        0,          %Enable%
HKR, Ndi\Params\Gather\enum,        "0",        0,          %Disable%

HKR, Ndi\Params\Offload.GuestCS,    ParamDesc,  0,          %GuestCS%
HKR, Ndi\Params\Offload.GuestCS,    Default,    0,          "0"
HKR, Ndi\Params\Offload.GuestCS,    type,       0,          "enum"
HKR, Ndi\Params\Offload.GuestCS\enum,"1",       0,          %Enable%
HKR, Ndi\Params\Offload.GuestCS\enum,"0",       0,          %Disable%

HKR, Ndi\Params\InterruptRecovery,  ParamDesc,  0,          %InterruptRecovery%
HKR, Ndi\Params\InterruptRecovery,  Default,    0,          "1"
HKR, Ndi\Params\InterruptRecovery,  type,       0,          "enum"
HKR, Ndi\Params\InterruptRecovery\enum,         "1",        0,  %Enable%
HKR, Ndi\Params\InterruptRecovery\enum,         "0",        0,  %Disable%

HKR, Ndi\params\NumberOfHandledRXPackersInDPC,       ParamDesc,  0,          %NumberOfHandledRXPackersInDPC%
HKR, Ndi\params\NumberOfHandledRXPackersInDPC,       type,       0,          "long"
HKR, Ndi\params\NumberOfHandledRXPackersInDPC,       default,    0,          "1000"
HKR, Ndi\params\NumberOfHandledRXPackersInDPC,       min,        0,          "1"
HKR, Ndi\params\NumberOfHandledRXPackersInDPC,       max,        0,          "10000"
HKR, Ndi\params\NumberOfHandledRXPackersInDPC,       step,       0,          "1"

HKR, Ndi\Params\PacketFilter,       ParamDesc,  0,          %PacketFilter%
HKR, Ndi\Params\PacketFilter,       Default,    0,          "1"
HKR, Ndi\Params\PacketFilter,       type,       0,          "enum"
HKR, Ndi\Params\PacketFilter\enum,  "1",        0,          %Enable%
HKR, Ndi\Params\PacketFilter\enum,  "0",        0,          %Disable%

HKR, Ndi\Params\BatchReceive,       ParamDesc,  0,          %BatchReceive%
HKR, Ndi\Params\BatchReceive,       Default,    0,          "1"
HKR, Ndi\Params\BatchReceive,       type,       0,          "enum"
HKR, Ndi\Params\BatchReceive\enum,  "1",        0,          %Enable%
HKR, Ndi\Params\BatchReceive\enum,  "0",        0,          %Disable%

HKR, Ndi\Params\Promiscuous,        ParamDesc,  0,          %Promiscuous%
HKR, Ndi\Params\Promiscuous,        Default,    0,          "0"
HKR, Ndi\Params\Promiscuous,        type,       0,          "enum"
HKR, Ndi\Params\Promiscuous\enum,   "1",        0,          %Enable%
HKR, Ndi\Params\Promiscuous\enum,   "0",        0,          %Disable%

HKR, Ndi\Params\IPPacketsCheck,     ParamDesc,  0,          %IPPacketsCheck%
HKR, Ndi\Params\IPPacketsCheck,     Default,    0,          "0"
HKR, Ndi\Params\IPPacketsCheck,     type,       0,          "enum"
HKR, Ndi\Params\IPPacketsCheck\enum,"0",        0,          %Disable%
HKR, Ndi\Params\IPPacketsCheck\enum,"1",        0,          %Tx%
HKR, Ndi\Params\IPPacketsCheck\enum,"2",        0,          %Rx%
HKR, Ndi\Params\IPPacketsCheck\enum,"3",        0,          %TxRx%

HKR, Ndi\Params\UseSwTxChecksum,    ParamDesc,  0,          %UseSwTxChecksum%
HKR, Ndi\Params\UseSwTxChecksum,    Default,    0,          "0"
HKR, Ndi\Params\UseSwTxChecksum,    type,       0,          "enum"
HKR, Ndi\Params\UseSwTxChecksum\enum,   "1",    0,          %Enable%
HKR, Ndi\Params\UseSwTxChecksum\enum,   "0",    0,          %Disable%

[kvmnet5.CopyFiles]
netkvm.sys,,,2

[kvmnet5.Service]
DisplayName     = %kvmnet5.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\netkvm.sys
LoadOrderGroup  = NDIS
AddReg          = TextModeFlags.Reg

[kvmnet5.EventLog]
AddReg = kvmnet5.AddEventLog.Reg

[kvmnet5.AddEventLog.Reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7

[TextModeFlags.Reg]
HKR, , TextModeFlags,    0x00010001, 0x0001

[SourceDisksNames]
1 = %DiskId1%,,,""

[SourceDisksFiles]
netkvm.sys  = 1,,

[DestinationDirs]
kvmnet5.CopyFiles = 12

[Strings]
VENDOR            = "INX_COMPANY"
kvmnet5.DeviceDesc   = "INX_PREFIX_VENDORVirtIO Ethernet Adapter"
kvmnet5.Service.DispName  = "INX_PREFIX_VENDORVirtIO Ethernet Adapter Service"
DiskId1 = "INX_PREFIX_VENDORVirtIO Ethernet Adapter Driver Disk #1"

NetworkAddress = "Assign MAC"
ConnectRate = "Init.ConnectionRate(Mb)"
Priority = "Init.Do802.1PQ"
MergeableBuf = "Init.UseMergedBuffers"
MTU = "Init.MTUSize"
Indirect = "Init.IndirectTx"
TxCapacity = "Init.MaxTxBuffers"
RxCapacity = "Init.MaxRxBuffers"
Offload.TxChecksum = "Offload.Tx.Checksum"
Offload.TxLSO = "Offload.Tx.LSO"
Offload.RxCS = "Offload.Rx.Checksum"
EnableLogging = "Logging.Enable"
DebugLevel = "Logging.Level"
LogStatistics = "Logging.Statistics(sec)"

ConnectAfter = "TestOnly.DelayConnect(ms)"
DPCCheck = "TestOnly.DPCChecking"
Gather = "TestOnly.Scatter-Gather"
GuestCS = "TestOnly.GuestChecksum"
InterruptRecovery = "TestOnly.InterruptRecovery"
PacketFilter = "TestOnly.HwPacketFilter"
BatchReceive = "TestOnly.BatchReceive"
Promiscuous = "TestOnly.Promiscuous"
IPPacketsCheck = "TestOnly.AnalyzeIPPackets"
NumberOfHandledRXPackersInDPC = "TestOnly.RXThrottle"
UseSwTxChecksum = "TestOnly.UseSwTxChecksum"
Tx = "Tx Enabled";
Rx = "Rx Enabled";
TxRx = "Rx & Tx Enabled";

Disable = "Disabled"
Enable  = "Enabled"
Enable* = "Enabled*"
String_16 = "16"
String_32 = "32"
String_64 = "64"
String_128 = "128"
String_256 = "256"
String_512 = "512"
String_1024 = "1024"
PriorityVlanTag = "Priority and VLAN tagging"
PriorityOnly = "Priority"
VLan = "VLan"
Priority_Vlan = "All"
10M = "10M"
100M = "100M"
1G   = "1G"
10G = "10G"
TCPv4 = "TCP(v4)"
TCPUDPv4 = "TCP/UDP(v4)"
TCPUDPAll = "TCP/UDP(v4,v6)"
All = "All"
IPv4 = "IPv4"
Maximal = "Maximal"

