;/*++
;
;INX_COPYRIGHT_1
;INX_COPYRIGHT_2
;
;Module Name:
;    BALLOON.INF
;
;Abstract:
;
;Installation Notes: 
;    Using Devcon: Type "devcon install BALLOON.inf PCI\VEN_1AF4&DEV_1002&SUBSYS_0005_INX_SUBSYS_VENDOR_ID&REV_00" or
;                       "devcon install BALLOON.inf PCI\VEN_1AF4&DEV_1045&SUBSYS_1100_INX_SUBSYS_VENDOR_ID&REV_01" to install
;
;--*/

[Version]
Signature="$WINDOWS NT$"
Class=System
ClassGuid={4d36e97d-e325-11ce-bfc1-08002be10318}
Provider=%VENDOR%
DriverVer=01/01/2008,0.0.0.1 ; this line will be replaced with stampinf
CatalogFile=Balloon.cat
DriverPackageType = PlugAndPlay
DriverPackageDisplayName = %BALLOON.DeviceDesc%
PnpLockdown = 1

[DestinationDirs]
DefaultDestDir = 12
BALLOON_Device_CoInstaller_CopyFiles = 11

[SourceDisksNames]
1 = %DiskId1%,,,""

[SourceDisksFiles]
balloon.sys  = 1,,
WdfCoInstaller$KMDFCOINSTALLERVERSION$.dll=1 ; make sure the number matches with SourceDisksNames

;*****************************************
; BALLOON  Install Section
;*****************************************

[Manufacturer]
%VENDOR%=Standard,NT$ARCH$

[Standard.NT$ARCH$]
%BALLOON.DeviceDesc%=BALLOON_Device, PCI\VEN_1AF4&DEV_1002&SUBSYS_0005_INX_SUBSYS_VENDOR_ID&REV_00, PCI\VEN_1AF4&DEV_1002
%BALLOON.DeviceDesc%=BALLOON_Device, PCI\VEN_1AF4&DEV_1045&SUBSYS_1100_INX_SUBSYS_VENDOR_ID&REV_01, PCI\VEN_1AF4&DEV_1045

[BALLOON_Device.NT]
CopyFiles=Drivers_Dir

[Drivers_Dir]
balloon.sys

[BALLOON_Device.NT.HW]
AddReg=BALLOON_SD

[BALLOON_SD]
HKR,,Security,,"D:P(A;;GA;;;SY)"

;-------------- Service installation
[BALLOON_Device.NT.Services]
AddService = BALLOON,%SPSVCINST_ASSOCSERVICE%, BALLOON_Service_Inst, BALLOON_Logging_Inst

; -------------- BALLOON driver install sections
[BALLOON_Service_Inst]
DisplayName    = %BALLOON.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START 
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\balloon.sys

; -------------- BALLOON driver eventlog install sections
[BALLOON_Logging_Inst]
AddReg = BALLOON_Logging_Inst_AddReg

[BALLOON_Logging_Inst_AddReg]
HKR,,EventMessageFile,0x00020000,"%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\System32\drivers\balloon.sys"
HKR,,TypesSupported,0x00010001,7

;--- BALLOON_Device Coinstaller installation ------
;

[BALLOON_Device.NT.CoInstallers]
AddReg=BALLOON_Device_CoInstaller_AddReg
CopyFiles=BALLOON_Device_CoInstaller_CopyFiles

[BALLOON_Device_CoInstaller_AddReg]
HKR,,CoInstallers32,0x00010000, "WdfCoInstaller$KMDFCOINSTALLERVERSION$.dll,WdfCoInstaller"

[BALLOON_Device_CoInstaller_CopyFiles]
WdfCoInstaller$KMDFCOINSTALLERVERSION$.dll

[BALLOON_Device.NT.Wdf]
KmdfService =  BALLOON, BALLOON_wdfsect
[BALLOON_wdfsect]
KmdfLibraryVersion = $KMDFVERSION$


[Strings]
SPSVCINST_ASSOCSERVICE= 0x00000002
VENDOR = "INX_COMPANY"
DiskId1 = "INX_PREFIX_VIRTIOVirtIO Balloon Installation Disk #1"
BALLOON.DeviceDesc = "INX_PREFIX_VIRTIOVirtIO Balloon Driver"
BALLOON.SVCDESC = "INX_PREFIX_VIRTIOVirtIO Balloon Service"
ClassName       = "INX_PREFIX_VIRTIOVirtIO Balloon Device"
